PDA INPUT AS a^nb^2n

